Product Name: SW-H411A HW Rev 1

MCU Version: v1.0.6a
GUI Version: v1.0.2
Release Date: 2021/12/27

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- Make sure that the unit is HW Rev 1. The sticker should not say HW Rev 2. 

----------------------------------------------------------
2. Revision History
----------------------------------------------------------
MCU v1.0.6a, GUI v1.0.2
- Bug fix for frontpanel hanging issue.
- Added "switchstable" and "switchfast" commands for higher compatibility. 
- Added support for TiGHT AV API.
- Updated GUI design.
- Bug fix for loosing IP Subnet and Gateway settings after power disconnect.
- Change to MCU v1.0.6a version number
- Change to GUI v1.0.2 version number


MCU v1.04
1. Optimize HDCP performance:
2. Add commands "HDCPON.","HDCPOFF.","HDCPBYPASS." and "STA_HDCP."
3. Adjust the priority level of RS232 port data handling function.
4. Change to V1.0.4 version number.
